• The LocoBuffer-USB operates at 57.6K baud speed.

• Connect the included USB cable to an unused USB port on your computer and
  to the LocoBuffer-USB. Your computer should detect the new unit and open a
  driver installation dialog.

• Two drivers will install. One appears under USB, 
  the other under Ports COM & LPT.

• Windows 8 and Windows 10 users must manually install the drivers for your 
  system from the included driver disk. See:
  http://www.rr-cirkits.com/win-8-driver-install.html
  http://www.rr-cirkits.com/win-10-driver-install.html

• Mac users choose the 'IMAC' folder, then the folder with your correct 
  OS X version, and run the included .dmg file.

• Linux users will automatically have the correct drivers pre-installed.

• The right hand green status indicator should illuminate as soon as your
  drivers are installed and they recognize the LocoBuffer-USB.

• Connect the unit's LocoNet® jack to any point on your system's LocoNet®. 
  The left hand green status indicator should illuminate, and the red activity
  indicator should now indicate all LocoNet® activity.

• Set your software's settings to match the communications port you just created.

• You should now be able to control your Railroad from your software. Call
  RR-CirKits at 1-704-843-3769 for further help.

• The information in the various directories in this folder is only needed if
  you do not have an internet connection, or if you have Windows 8 or Windows 10.
